DICOM PS3.7 2016c - Message Exchange

C.5.20 No Such SOP Class
Prev | C.5 Failure Status Class | Next

### C.5.20 No Such SOP Class

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Affected SOP Class UID | (0000,0002) | UI | 1 | This optional field contains the SOP Class UID that does not exist.
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0118H.

Prev | Up | Next
C.5.19 No Such SOP Instance | Home | C.5.21 Processing Failure

DICOM PS3.7 2016c - Message Exchange