DICOM PS3.17 2016c - Explanatory Information

XXX.3.9.3.4 Presentation Animation Module Recommendations
Prev | XXX.3.9.3 Encoding Details | Next

##### XXX.3.9.3.4 Presentation Animation Module Recommendations

This Module is replicated in each of the created Volumetric Presentation States.

Table XXX.3.9-4. Presentation Animation Module Recommendations

Attribute Name | Tag | Comment
--- | --- | ---
Presentation Animation Style | (0070,1A01) | Set to "INPUT_SEQ"
Recommended Animation Rate | (0070,1A03) | Set to "4" (steps per second)

Prev | Up | Next
XXX.3.9.3.3 Presentation View Description Module Recommendations | Home | XXX.4 Uses of Presentation View Description in the Identification Module

DICOM PS3.17 2016c - Explanatory Information