DICOM PS3.3 2016c - Information Object Definitions

C.8.24.4 IVUS Image Module
Prev | C.8.24 Enhanced US Volume Modules and Functional Group Macros | Next

#### C.8.24.4 IVUS Image Module

Table C.8.24.4-1 specifies the Attributes of an IVUS Module.

Table C.8.24.4-1. IVUS Image Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
IVUS Acquisition | (0018,3100) | 1 | Defined Terms: MOTOR_PULLBACK MANUAL_PULLBACK SELECTIVE GATED_PULLBACK See Section C.8.5.6.1.21
IVUS Pullback Rate | (0018,3101) | 1C | Required if IVUS Acquisition (0018,3100) value is MOTOR_PULLBACK. Specified in units of mm/sec. See Section C.8.5.6.1.22
IVUS Gated Rate | (0018,3102) | 1C | Required if IVUS Acquisition (0018,3100) value is GATED_PULLBACK. Specified in units of mm/beat. See Section C.8.5.6.1.23
IVUS Pullback Start Frame Number | (0018,3103) | 1C | Required if IVUS Acquisition (0018,3100) value is MOTOR_PULLBACK or GATED_PULLBACK. See Section C.8.5.6.1.24
IVUS Pullback Stop Frame Number | (0018,3104) | 1C | Required if IVUS Acquisition (0018,3100) value is MOTOR_PULLBACK or GATED_PULLBACK. See Section C.8.5.6.1.25

Prev | Up | Next
C.8.24.3.4 Transducer Description | Home | C.8.24.5 Excluded Intervals Module

DICOM PS3.3 2016c - Information Object Definitions