DICOM PS3.16 2016c - Content Mapping Resource

TID 5204 Wall Motion Analysis
Prev | Echocardiography Procedure Report Templates | Next

### TID 5204 Wall Motion Analysis

The Wall Motion Analysis Template is used to document wall motion scoring for any imaging modality.

Table TID 5204. Parameters

Parameter Name | Parameter Usage
--- | ---
$Procedure | The imaging procedure used for wall motion analysis.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 5204. Wall Motion Analysis

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (121070, DCM, "Findings") | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (121058, DCM, "Procedure reported") | 1 | M |  | $Procedure
3 | > | HAS ACQ CONTEXT | CODE | EV (18139-6, LN, "Stage") | 1 | U |  | BCID 3207 “Stress Test Procedure Phases”
4 | > | CONTAINS | IMAGE | EV (125201, DCM, "Illustration of Finding") | 1 | U |  |
5 | > | CONTAINS | TEXT | EV (18118-0, LN, "LV Wall Motion Segmental Findings") | 1 | U |  |
6 | > | CONTAINS | NUM | DT (125202, DCM, "LV Wall Motion Score Index") | 1 | U |  |
7 | >> | HAS CONCEPT MOD | CODE | EV (G-E048, SRT, "Assessment Scale") | 1 | M |  | BCID 12238 “Wall Motion Scoring Schemes”
8 | > | CONTAINS | CONTAINER | EV (121070, DCM, "Findings") | 1 | U |  |
9 | >> | HAS CONCEPT MOD | CODE | EV (G-C0E3, SRT, "Finding Site") | 1 | M |  | DT (T-D0772, SRT, "Myocardial Wall")
10 | >> | CONTAINS | CODE | EV (18179-2, LN, "Wall Segment") | 1-n | M |  | BCID 3717 “Myocardial Wall Segments”
11 | >>> | HAS PROPERTIES | CODE | EV (F-32050, SRT, "Cardiac Wall Motion") | 1 | MC | IF row 12 is absent | DCID 3703 “Wall Motion”
12 | >>> | HAS PROPERTIES | CODE | EV (G-C504, SRT, "Associated Morphology") | 1 | MC | IF row 11 is absent | DCID 3704 “Myocardium Wall Morphology Findings”
13 | >>> | HAS PROPERTIES | NUM | DT (G-C1E3, SRT, "Score") | 1 | U |  |
14 | >>> | HAS PROPERTIES | NUM | EV (122624, DCM, "Wall Thickness Ratio end-systolic to end-diastolic") | 1 | U |  | UNITS = DT (%, UCUM, "%")

Content Item Descriptions

Row 3 | The stage of the protocol at which these findings were scored. This row may be absent if this is a generic, non-staged scoring.
Row 4 | Image that graphically depicts the segments and their scores.
Row 5 | Text narration accompanying this stage.
Row 6 | The composite score computed from the average of the scored segments
Row 7 | The type of scoring scheme used to score this exam.
Row 8 | A container of all of the individual segment findings for this stage. The container shall be present if the observer makes an assessment, including the assessment of Not Visualized. It shall not be present if no evaluation was made.
Rows 11, 12 | Scar/thinning (in Row 12) may accompany akinesis and dyskinesis (in Row 11).
Row 13 | A numeric designation for the score. Score ranges vary, typically 0-4 or 0-5. Numeric scores may depend on wall motion findings as well as morphology findings. See Table 5204-1 for conventional numeric assignment schemes. The UCUM annotation code enables specifying the numeric range, ({L:N}, UCUM, "scale L:N"), where L and N are the lower and upper ends of the range.

A description of the scoring schemes described in Table 5204-1 is available in Recommendations for Quantitation of the Left Ventricle by Two-Dimensional Echocardiography, Journal of the American Society of Echocardiography, Vol 2, No 5 358-367, Oct 1989.

Table 5204-1. Numeric Score Assignment for Segmental Findings

Conventional Numeric Assignment | Wall Motion Finding or Morphology Finding
--- | ---
4 Point | 5 Point | 5 Point with Graded Hypokinesis
-1 | (F-32050, SRT, "Cardiac Wall Motion") = (R-0030D, SRT, "Hyperkinesis") | (F-32050, SRT, "Cardiac Wall Motion") = (R-0030D, SRT, "Hyperkinesis") | (F-32050, SRT, "Cardiac Wall Motion") = (R-0030D, SRT, "Hyperkinesis")
0 | (F-32050, SRT, "Cardiac Wall Motion") = (122288, DCM, "Not Visualized") | (F-32050, SRT, "Cardiac Wall Motion") = (122288, DCM, "Not Visualized") | (F-32050, SRT, "Cardiac Wall Motion") = (122288, DCM, "Not Visualized")
1 | (F-32050, SRT, "Cardiac Wall Motion") = (R-00344, SRT, "Normal Wall Motion") | (F-32050, SRT, "Cardiac Wall Motion") = (R-00344, SRT, "Normal Wall Motion") | (F-32050, SRT, "Cardiac Wall Motion") = (R-00344, SRT, "Normal Wall Motion")
1.5 |  |  | (F-32050, SRT, "Cardiac Wall Motion") = (R-00327, SRT, "Mild Hypokinesis")
2 | (F-32050, SRT, "Cardiac Wall Motion") = (F-32056, SRT, "Hypokinesis") | (F-32050, SRT, "Cardiac Wall Motion") = (F-32056, SRT, "Hypokinesis") | (F-32050, SRT, "Cardiac Wall Motion") = (R-0032F, SRT, "Moderate Hypokinesis")
2.5 |  |  | (F-32050, SRT, "Cardiac Wall Motion") = (R-00370, SRT, "Severe Hypokinesis")
3 | (F-32050, SRT, "Cardiac Wall Motion") = (F-30004, SRT, "Akinesis") | (F-32050, SRT, "Cardiac Wall Motion") = (F-30004, SRT, "Akinesis") | (F-32050, SRT, "Cardiac Wall Motion") = (F-30004, SRT, "Akinesis")
4 | (F-32050, SRT, "Cardiac Wall Motion") = (F-32052, SRT, "Dyskinesis") | (F-32050, SRT, "Cardiac Wall Motion") = (F-32052, SRT, "Dyskinesis") | (F-32050, SRT, "Cardiac Wall Motion") = (F-32052, SRT, "Dyskinesis")
5 |  | (G-C504, SRT, "Associated Morphology") = (D3-10510, SRT, "Ventricular Aneurysm") | (G-C504, SRT, "Associated Morphology") = (D3-10510, SRT, "Ventricular Aneurysm")

Prev | Up | Next
TID 5203 Echo Measurement | Home | TID 5220 Pediatric, Fetal and Congenital Cardiac Ultrasound Reports

DICOM PS3.16 2016c - Content Mapping Resource