DICOM PS3.7 2016d - Message Exchange

C.4.2 Attribute List Error
Prev | C.4 Warning Status Class | Next

### C.4.2 Attribute List Error

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Affected SOP Class UID | (0000,0002) | UI | 1 | This optional field contains the SOP Class UID for which Attributes were not recognized.
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0107H.
Affected SOP Instance UID | (0000,1000) | UI | 1 | This optional field contains the UID of the SOP Instance for which Attributes were not recognized.
Attribute Identifier List | (0000,1005) | AT | 1-n | This optional field contains an Attribute Tag for each Attribute that was not recognized.

Prev | Up | Next
C.4 Warning Status Class | Home | C.4.3 Attribute Value Out of Range

DICOM PS3.7 2016d - Message Exchange