DICOM PS3.4 2016d - Service Class Specifications

P.2.2.3 Service Class Provider Behavior
Prev | P.2.2 Operation | Next

#### P.2.2.3 Service Class Provider Behavior

The SCP shall manage the creation of SOP Instances of the Procedure Log Storage Service. It shall receive, via the N-ACTION request primitive, requests for logging of events that occur during a Study. The SCP shall (consonant with application dependent constraints) incorporate those event records into a Procedure Log SOP Instance for the specified Study.

The SCP shall return, via the N-ACTION response primitive, the N-ACTION Response Status Code applicable to the associated action request.

Prev | Up | Next
P.2.2.2 Service Class User Behavior | Home | P.2.2.4 Status Codes

DICOM PS3.4 2016d - Service Class Specifications