DICOM PS3.16 2016d - Content Mapping Resource

TID 3219 Segment Values
Prev | Quantitative Arterial Analysis Report SR IOD Templates | Next

### TID 3219 Segment Values

The Segment Values Template consists of Content Items providing quantitative arterial analysis measurements for a total analyzed segment or sub segment.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 3219. Segment Values

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (122510, DCM, "Length Luminal Segment") $Unit = DT (mm, UCUM, "mm")
2 |  | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (G-0364, SRT, "Vessel Luminal Diameter") $Derivation = EV (R-404FB, SRT, "Minimum") $Unit = DT (mm, UCUM, "mm")
3 |  | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (G-0364, SRT, "Vessel Luminal Diameter") $Derivation = EV (G-A437, SRT, "Maximum") $Unit = DT (mm, UCUM, "mm")
4 |  | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (G-0364, SRT, "Vessel Luminal Diameter") $Derivation = EV (R-00317, SRT, "Mean") $Unit = DT (mm, UCUM, "mm")
5 |  | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = EV (G-0364, SRT, "Vessel Luminal Diameter") $Derivation = EV (R-10047, SRT, "Standard Deviation") $Unit = DT (mm, UCUM, "mm")

Content Item Descriptions

Row 1 | Measured along the midline of the left and right contour.

Prev | Up | Next
TID 3218 Position in Arterial Segment | Home | IVUS Report Templates

DICOM PS3.16 2016d - Content Mapping Resource