DICOM PS3.2 2016e - Conformance

G.4.2.2.3 Association Initiation Policy
Prev | G.4.2.2 STORAGE-SCU | Next

##### G.4.2.2.3 Association Initiation Policy

STORAGE-SCU attempts to initiate a new association for each instance it attempts to transfer.

###### G.4.2.2.3.1 Activity - Send Storage Request

###### G.4.2.2.3.1.1 Description and Sequencing of Activities

For each Image, Presentation State, or Hanging Protocol Instance selected from the user interface to be transferred, a single attempt will be made to transmit it to the selected remote AE. If the send fails, for whatever reason, no retry will be performed, and an attempt will be made to send the next instance.

###### G.4.2.2.3.1.2 Proposed Presentation Contexts

Table G.4.2-11. Proposed Presentation Contexts for STORAGE-SCU and Receive Storage Request

Presentation Context Table
Abstract Syntax | Transfer Syntax | Role | Extended Negotiation
--- | --- | --- | ---
Name | UID | Name List | UID List
See Table G.4.2-7 | See Table G.4.2-7 | Implicit VR Little Endian | 1.2.840.10008.1.2 | SCU | None
Explicit VR Little Endian | 1.2.840.10008.1.2.1

STORAGE-SCU will propose Presentation Contexts only for the SOP Class of the instance that is to be transferred.

For that SOP Class, STORAGE-SCU will propose multiple Presentation Contexts, one for each of the supported Transfer Syntaxes, and an additional Presentation Context with all of the supported Transfer Syntaxes, in order to determine which Transfer Syntaxes the remote SCP supports, and which it prefers.

###### G.4.2.2.3.1.2.1 Extended Negotiation

No extended negotiation is performed.

###### G.4.2.2.3.1.3 SOP Specific Conformance

###### G.4.2.2.3.1.3.1 SOP Specific Conformance to Storage Service Class

STORAGE-SCU provides standard conformance to the Storage Service Class.

###### G.4.2.2.3.1.3.2 SOP Specific Conformance to Hanging Protocol Storage Service Class

STORAGE-SCU provides standard conformance to the Hanging Protocol Storage Service Class.

In Hanging Protocol Instances created on the Viewer, no Private Attributes are used as the value of Selector Attribute (0072,0026) in any of the Sequence Attributes to which it applies.

###### G.4.2.2.3.1.3.3 Presentation Context Acceptance Criterion

STORAGE-SCU does not accept associations.

###### G.4.2.2.3.1.3.4 Transfer Syntax Selection Policies

STORAGE-SCU prefers explicit Transfer Syntaxes. If offered a choice of Transfer Syntaxes in the accepted Presentation Contexts, it will apply the following priority to the choice of Presentation Context to use for the C-STORE operation:

1. first encountered explicit Transfer Syntax,

2. default Transfer Syntax.

###### G.4.2.2.3.1.3.5 Response Status

STORAGE-SCU will behave as described in the Table below in response to the status returned in the C-STORE response command message.

Table G.4.2-12. Response Behavior for STORAGE-SCU and Send Storage Request

Service Status | Further Meaning | Status Codes | Behavior
--- | --- | --- | ---
Failure | Refused: Out of Resources | A7xx | The user is notified and the failure is logged
| Error: Data Set does not match SOP Class | A9xx | The user is notified and the failure is logged
| Error: Cannot understand | Cxxx | The user is notified and the failure is logged
Warning | Coercion of Data Elements | B000 | Ignored
| Data Set does not match SOP Class | B007 | Ignored
| Elements Discarded | B006 | Ignored
Success |  | 0000 | Ignored

Prev | Up | Next
G.4.2.2.2 Association Policies | Home | G.4.2.2.4 Association Acceptance Policy

DICOM PS3.2 2016e - Conformance