DICOM PS3.18 2016e - Web Services

6.9.3.3.3 Response Message
Prev | 6.9.3.3 Response | Next

##### 6.9.3.3.3 Response Message

The response message body contains the results.

The format of the response message body shall contain one of the Media Types specified by the request Accept header field. An Origin-Server shall support all Media-Types allowed in the request.

###### 6.9.3.3.3.1 XML Response Message

- Content-Type:

  - multipart/related; type="application/dicom+xml"

- The response is a multipart message body where each part is a DICOM PS3.19 XML DicomNativeModel element containing the attributes for one matching UPS Instance (see Section A.1 in PS3.19 ).

- If there are no matching results, the message body shall be empty.

- Each part in the multipart body includes the following HTTP headers:

  - Content-Type: application/dicom+xml

###### 6.9.3.3.3.2 JSON Response Message

- Content-Type:

  - application/dicom+json

- The response is a DICOM JSON message containing a DICOM JSON property for each matching UPS Instance containing sub-properties describing the matching attributes for each UPS Instance (see Section F.2).

- If there are no matching results, the JSON message shall be empty.

Prev | Up | Next
6.9.3.3.2 Query Result Attribute | Home | 6.9.4 RetrieveUPS

DICOM PS3.18 2016e - Web Services