DICOM PS3.3 2016e - Information Object Definitions

A.28.4 Overlay Plane Module
Prev | A.28 Digital Intra-Oral X-Ray Image IOD | Next

### A.28.4 Overlay Plane Module

If the Overlay Plane Module is present, any Overlays defined in that Module shall store the overlay data in Overlay Data (60xx,3000), and not any unused high bits in Pixel Data (7FE0,0010).

Prev | Up | Next
A.28.3 Digital Intra-Oral X-Ray Image IOD Module Table | Home | A.29 RT Beams Treatment Record IOD

DICOM PS3.3 2016e - Information Object Definitions