DICOM PS3.11 2016e - Media Storage Application Profiles

H.3.5 Security Parameters
Prev | H.3 STD-GEN-DVD and STD-GEN-SEC-DVD Profile Classes | Next

### H.3.5 Security Parameters

The STD-GEN-SEC-DVD application profiles require that all DICOM Files in the File-set including the DICOMDIR be Secure DICOM Files encapsulated in accordance with the requirements of the Basic DICOM Media Security Profile as defined in PS3.15.

### Note

These Application Profiles do not place any consistency restrictions on the use of the Basic DICOM Media Security Profile with different DICOM Files of one File-set. For example, readers should not assume that all Files in the File-set can be decoded by the same set of recipients. Readers should also not assume that all secure Files use the same approach (hash key or digital signature) to ensure Integrity or carry the same originators' signatures.

Prev | Up | Next
H.3.4 Other Parameters | Home | I DVD MPEG2 Interchange Profiles (Normative)

DICOM PS3.11 2016e - Media Storage Application Profiles