DICOM PS3.3 2016e - Information Object Definitions

C.8.8.15.9 Control Point Relative Position
Prev | C.8.8.15 RT Brachy Application Setups Module | Next

##### C.8.8.15.9 Control Point Relative Position

Control Point Relative Position (300A,02D2) shall describe where a given source in a channel is located with respect to the end of the channel. This position shall correspond to the end of the afterloader applicator, not the "safe position".

Prev | Up | Next
C.8.8.15.8 Source Transit Time | Home | C.8.8.15.10 Control Point 3D Position

DICOM PS3.3 2016e - Information Object Definitions