DICOM PS3.17 2016e - Explanatory Information

HHH.3.3.2 DICOM (Encoded Content) Requester
Prev | HHH.3.3 Description of The Use Cases | Next

#### HHH.3.3.2 DICOM (Encoded Content) Requester

1. The requesting system is an application capable of making Web Service requests and able to process data encoded as a DICOM File, per DICOM PS3.10 encodings.

2. Reference information may come in a wide variety of forms. It is expected to include at least the Study UID, Series UID, and Individual SOP instance information. This may be encoded as part of an HL7 reference within a CDA document, a DICOM SOP Instance reference, or other formats.

3. The request specifies

   1. Requested Data set

      1. Study UID

      2. List of Series UID

      3. List of SOP Instance UIDs

   2. Optionally, it may also specify subset information

      1. Instance and Frame Level Retrieve SOP classes subset information for selecting frames

      2. No-pixel data request (using the Transfer Syntax parameter)

      3. Anonymization

4. The response provides

   1. SOP Instances, encoded per DICOM PS3.10.

Prev | Up | Next
HHH.3.3 Description of The Use Cases | Home | HHH.3.3.3 Rendered (JPEG/PDF) Requester

DICOM PS3.17 2016e - Explanatory Information