DICOM PS3.16 2016e - Content Mapping Resource

TID 3504 Arterial Pressure Measurement
Prev | Hemodynamics Report Templates | Next

### TID 3504 Arterial Pressure Measurement

The Arterial Pressure Measurement Template consists of a CONTAINER, with an acquisition context of the measurement anatomic site, and containing systolic, diastolic, and mean measurements. This implies that the name of the measurement is effectively post-coordinated from the measurement name, the Hemodynamic Measurement Group container (procedure phase) name, and the acquisition context (finding site) value.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 3504. Arterial Pressure Measurement

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (P2-36102, SRT, "Arterial pressure measurements") | 1 | M |  |
2 | > |  | INCLUDE | DTID 3530 “Hemodynamic Acquisition Context” | 1 | M |  | $LocationName = EV (G-C0E3, SRT, "Finding Site") $LocationValue = DCID 3606 “Arterial Source Locations”
3 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (8480-6, LN, "Intravascular arterial Systolic pressure") $Units = DCID 3500 “Pressure Units”
4 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (8462-4, LN, "Intravascular arterial Diastolic pressure") $Units = DCID 3500 “Pressure Units”
5 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (8478-0, LN, "Intravascular arterial mean pressure") $Units = DCID 3500 “Pressure Units”
6 | > | CONTAINS | INCLUDE | DTID 3550 “Pressure Waveform Measurements” | 1-n | U |  |

Prev | Up | Next
TID 3501 Hemodynamics Measurement Group | Home | TID 3505 Atrial Pressure Measurement

DICOM PS3.16 2016e - Content Mapping Resource