DICOM PS3.4 2017a - Service Class Specifications

I.3.4 Conformance Statement Requirements
Prev | I.3 Conformance | Next

### I.3.4 Conformance Statement Requirements

An implementation of the Media Storage Service Class may support one or more Roles as specified in Table I.3-1. In addition, the implementation may conform to one or more of the SOP Classes of the Media Storage Service Class defined in Section I.4. The Conformance Statement shall be in the format defined by PS3.2.

Table I.3-1. Allowed Combinations of Roles

Roles | FSR | FSC | FSU
--- | --- | --- | ---
With a Directory Information Module | Allowed | Allowed | Allowed Directory shall be updated
With no Directory Information Module | Allowed | Allowed | Allowed Directory shall not be updated

The following aspects shall be documented in the Conformance Statement of any implementation claiming conformance to one of the Media Storage SOP Classes:

- the subset of the Basic Directory Information Object Model supported;

- When the Directory Information Module is created or updated (Directory Information Module supported), the optional standard keys that may be included in Directory Records shall be documented. Private Keys and Private Records may also be documented;

Prev | Up | Next
I.3.3 Conformance as an FSU | Home | I.3.5 Standard Extended, Specialized, and Private Conformance

DICOM PS3.4 2017a - Service Class Specifications