DICOM PS3.3 2017a - Information Object Definitions

A.20.3 RT Plan IOD Module Table
Prev | A.20 RT Plan IOD | Next

### A.20.3 RT Plan IOD Module Table

Table A.20.3-1 specifies the Modules of the RT Plan IOD.

Table A.20.3-1. RT Plan IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | RT Series | C.8.8.1 | M
Clinical Trial Series | C.7.3.2 | U
Frame of Reference | Frame of Reference | C.7.4.1 | U
Equipment | General Equipment | C.7.5.1 | M
Plan | RT General Plan | C.8.8.9 | M
RT Prescription | C.8.8.10 | U
RT Tolerance Tables | C.8.8.11 | U
RT Patient Setup | C.8.8.12 | U
RT Fraction Scheme | C.8.8.13 | U
RT Beams | C.8.8.14 | C - Required if RT Fraction Scheme Module exists and Number of Beams (300A,0080) is greater than zero for one or more fraction groups. Shall not be present, if RT Brachy Application Setups Module is present. May be present otherwise.
RT Brachy Application Setups | C.8.8.15 | C - Required if RT Fraction Scheme Module exists and Number of Brachy Application Setups (300A,00A0) is greater than zero for one or more fraction groups. Shall not be present, if RT Beams Module is present. May be present otherwise.
Approval | C.8.8.16 | U
General Reference | C.12.4 | U
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U

### Note

1. Retired. See PS3.3-2011.

2. The Audio Module (Retired) was previously included in this IOD but has been retired. See PS3.3-2004.

#### A.20.3.1 RT Fraction Scheme Module

The RT Fraction Scheme Module is structured to be used together with the RT Beams Module or RT Brachy Application Setups Module. If beams are referenced in the RT Fraction Scheme Module, all such beams shall be included in the RT Beams Module if it is present. Similarly, if brachy application setups are referenced in the RT Fraction Scheme Module, all such setups shall be included in the RT Brachy Application Setups Module if it is present. However, the RT Fraction Scheme Module can be used without the RT Beams Module or RT Brachy Application Setups Module if no beams or brachy application setups are referenced, and the RT Beams Module or RT Brachy Application Setups Module can also be used without the RT Fraction Scheme Module if no fraction scheme information is available.

Prev | Up | Next
A.20.2 RT Plan IOD Entity-Relationship Model | Home | A.20.3.2 RT Prescription Module

DICOM PS3.3 2017a - Information Object Definitions