DICOM PS3.16 2017a - Content Mapping Resource

TID 3102 Waveform Acquisition
Prev | Procedure Log IOD Templates | Next

### TID 3102 Waveform Acquisition

The Waveform Acquisition Template allows recording of the essential parameters of a digital waveform acquired during the procedure.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 3102. Waveform Acquisition

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | WAVEFORM | EV (121143, DCM, "Waveform Acquired") | 1 | M |  |
2 | > | HAS ACQ CONTEXT | CODE | EV (121139, DCM, "Modality") | 1 | M |  | DCID 29 “Acquisition Modality” Derived from referenced waveform SOP Instance attribute (0008,0060)
3 | > | HAS ACQ CONTEXT | NUM | EV (121142, DCM, "Acquisition Duration") | 1 | U |  |
4 | > |  | INCLUDE | DTID 3010 “Log Entry Qualifiers” | 1 | U |  |

Prev | Up | Next
TID 3101 Image Acquisition | Home | TID 3103 Referenced Object

DICOM PS3.16 2017a - Content Mapping Resource