DICOM PS3.4 2017b - Service Class Specifications

P.2.2.2 Service Class User Behavior
Prev | P.2.2 Operation | Next

#### P.2.2.2 Service Class User Behavior

The SCU shall request logging of events that occur during a Study, using the N-ACTION request primitive.

The SCU shall receive N-ACTION responses. The actions taken upon a response status of Failure, or upon non-response of the SCP, are implementation dependent.

Prev | Up | Next
P.2.2 Operation | Home | P.2.2.3 Service Class Provider Behavior

DICOM PS3.4 2017b - Service Class Specifications