DICOM PS3.11 2017b - Media Storage Application Profiles

N.3.2 Physical Medium and Medium Format
Prev | N.3 STD-GEN-BD-MPEG4-LV42 and STD-GEN-SEC-BD-MPEG4-LV42 Profile Classes | Next

### N.3.2 Physical Medium and Medium Format

The STD-GEN-BD-MPEG4-LV42 and STD-GEN-SEC-BD-MPEG4-LV42 application profiles require any of the 120 mm BD media, as defined in PS3.12.

Prev | Up | Next
N.3 STD-GEN-BD-MPEG4-LV42 and STD-GEN-SEC-BD-MPEG4-LV42 Profile Classes | Home | N.3.3 Directory Information in DICOMDIR

DICOM PS3.11 2017b - Media Storage Application Profiles