DICOM PS3.16 2017b - Content Mapping Resource

TID 10004 Accumulated Fluoroscopy and Acquisition Projection X-Ray Dose
Prev | X-Ray Radiation Dose SR IOD Templates | Next

### TID 10004 Accumulated Fluoroscopy and Acquisition Projection X-Ray Dose

This general Template provides detailed information on projection X-Ray dose value accumulations over several irradiation events from the same equipment (typically a study or a performed procedure step).

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 10004. Accumulated Fluoroscopy and Acquisition Projection X-Ray Dose

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | NUM | EV (113726, DCM, "Fluoro Dose Area Product Total") | 1 | MC | IFF TID (10003) Row 7 value = (P5-06000, SRT, "Fluoroscopy") for at least one irradiation event | UNITS = EV (Gy.m2, UCUM, "Gy.m2")
2 |  |  | NUM | EV (113728, DCM, "Fluoro Dose (RP) Total") | 1 | MC | IFF TID (10003) Row 7 value = (P5-06000, SRT, "Fluoroscopy") for at least one irradiation event AND any of the values of TID (10001) Row 18 are not (113858, DCM, "MPPS Content"). | UNITS = EV (Gy, UCUM, "Gy")
3 |  |  | NUM | EV (113730, DCM, "Total Fluoro Time") | 1 | MC | IFF TID (10003) Row 7 value = (P5-06000, SRT, "Fluoroscopy") for at least one irradiation event. | UNITS = EV (s, UCUM, "s")
4 |  |  | NUM | EV (113727, DCM, "Acquisition Dose Area Product Total") | 1 | MC | IF any of the values of TID (10001) Row 18 are not (113858, DCM, "MPPS Content"). | UNITS = EV (Gy.m2, UCUM, "Gy.m2")
5 |  |  | NUM | EV (113729, DCM, "Acquisition Dose (RP) Total") | 1 | MC | IF any of the values of TID (10001) Row 18 are not (113858, DCM, "MPPS Content"). | UNITS = EV (Gy, UCUM, "Gy")
6 |  |  | NUM | EV (113855, DCM, "Total Acquisition Time") | 1 | MC | IF any of the values of TID (10001) Row 18 are not (113858, DCM, "MPPS Content"). | UNITS = EV (s, UCUM, "s")

Content Item Descriptions

Rows 1-3 | Fluoroscopic component only
Row 3 | Total clock time of Fluoroscopy accumulated over the defined scope of accumulation (i.e., the sum of the Irradiation Duration values for accumulated fluoroscopy irradiation events)
Rows 4-6 | Acquisition component only
Row 6 | Total clock time of acquisitions accumulated over the defined scope of accumulation (i.e., the sum of the Irradiation Duration values for accumulated acquisition irradiation events)

Prev | Up | Next
TID 10003C Irradiation Event X-Ray Mechanical Data | Home | TID 10005 Accumulated Mammography X-Ray Dose

DICOM PS3.16 2017b - Content Mapping Resource