DICOM PS3.16 2017b - Content Mapping Resource

CID 3263 Electrode Placement Values
Prev | B DCMR Context Groups (Normative) | Next

## CID 3263 Electrode Placement Values

This Context Group comprises the ECG lead placement system identifiers of ISO/IEEE 11073-10102. The terms included in the table below may not constitute the complete list; see the ISO/IEEE Standard.

### Note

Codes reprinted by permission of IEEE, Copyright 2004 by IEEE. ISO/IEEE 11073-10102 available through http://standards.ieee.org/.

Type:

  Extensible

Version:

  20080927

Table CID 3263. Electrode Placement Values

Coding Scheme Designator | Code Value | Code Meaning | ISO/IEEE 11073 MDC Equivalent Reference ID (Informative)
--- | --- | --- | ---
MDC | 10:11264 | Unspecified 12-lead system | MDC_ECG_LDSYS_12LD_UNSPECIFIED
MDC | 10:11265 | Standard 12-lead positions, electrodes placed individually | MDC_ECG_LDSYS_12LD_STD
MDC | 10:11266 | Mason-Likar lead positions, electrodes placed individually | MDC_ECG_LDSYS_12LD_MASON_LIKAR
MDC | 10:11267 | Mason-Likar lead positions, V1-V6 in electrode pad | MDC_ECG_LDSYS_12LD_VPAD
MDC | 10:11268 | 12-lead electrode pad | MDC_ECG_LDSYS_12LD_PAD
MDC | 10:11269 | 12-lead derived from Frank XYZ leads | MDC_ECG_LDSYS_12LD_FROM_FRANK
MDC | 10:11270 | 12-lead derived from non-standard leads | MDC_ECG_LDSYS_12LD_NON_STANDARD
MDC | 10:11271 | 12-lead for bicycle exercise testing, limb leads on back of patient | MDC_ECG_LDSYS_12LD_BICYCLE
MDC | 10:11272 | Standard 12-lead positions one intercostal space higher | MDC_ECG_LDSYS_12LD_RAISED_INTERCOSTAL
MDC | 10:11273 | Unspecified XYZ lead system | MDC_ECG_LDSYS_XYZ_UNSPECIFIED
MDC | 10:11274 | Frank XYZ lead system | MDC_ECG_LDSYS_XYZ_FRANK
MDC | 10:11275 | McFee-Parungao XYZ lead system | MDC_ECG_LDSYS_XYZ_MCFEE_PARUNAGO
MDC | 10:11276 | Cube XYZ lead system | MDC_ECG_LDSYS_XYZ_CUBE
MDC | 10:11277 | Bipolar uncorrected XYZ lead system | MDC_ECG_LDSYS_XYZ_BIPOLAR
MDC | 10:11278 | Pseudo-orthogonal XYZ lead system | MDC_ECG_LDSYS_XYZ_PSEUDO_ORTH
MDC | 10:11279 | XYZ leads derived from standard 12-lead | MDC_ECG_LDSYS_XYZ_FROM_12LD
MDC | 10:11280 | NEHB lead system | MDC_ECG_LDSYS_3LD_NEHB
MDC | 10:11281 | 3-lead system, CC5-CM5-ML | MDC_ECG_LDSYS_3LD_CC5_CM5_ML
MDC | 10:11282 | 3-lead system, CC5-CM5-CH5 | MDC_ECG_LDSYS_3LD_CM5_CC5_CH5
MDC | 10:11283 | 12-lead from Frank leads XYZ leads by Dower transformation | MDC_ECG_LDSYS_12LD_FROM_DOWER
MDC | 10:11284 | 12-lead from EASI leads (ES, AS, AI) by Dower/EASI transformation | MDC_ECG_LDSYS_12LD_FROM_EASI
MDC | 10:11285 | 12-lead from Limb Leads (I, II) and one or more V leads | MDC_ECG_LDSYS_12LD_FROM_LIMB
MDC | 10:11286 | Standard 12-lead and XYZ | MDC_ECG_LDSYS_12LD_STD_AND_XYZ
MDC | 10:11287 | Standard 12-lead and NEHB | MDC_ECG_LDSYS_12LD_STD_AND_NEHB
MDC | 10:11288 | Standard 12-lead and CC5-CM5-ML | MDC_ECG_LDSYS_12LD_STD_AND_CC5_CM5_ML
MDC | 10:11289 | Standard 12-lead and CM5-CC5-CH5 | MDC_ECG_LDSYS_12LD_STD_AND_CM5_CC5_CH5
MDC | 10:11290 | Standard 12-lead with extra leads to the right and/or left sides | MDC_ECG_LDSYS_12LD_STD_EXTD
MDC | 10:11291 | Standard 12-lead extended to the right by V5R, V4R, V3R | MDC_ECG_LDSYS_12LD_STD_EXTD_RIGHT
MDC | 10:11292 | Standard 12-lead extended to the left by V7, V8, V9 | MDC_ECG_LDSYS_12LD_STD_EXTD_LEFT

### Note

A prior version of this context group used codes from the SCP-ECG vocabulary.

Prev | Up | Next
CID 3262 ECG Patient State Values | Home | CID 3264 XYZ Electrode Placement Values (Retired)

DICOM PS3.16 2017b - Content Mapping Resource