DICOM PS3.4 2017b - Service Class Specifications

H.3.4 Conformance Statement
Prev | H.3 Print Management Conformance | Next

### H.3.4 Conformance Statement

The implementation Conformance Statement of these SOP Classes shall follow PS3.2.

The SCU Conformance Statement shall specify the following items:

- maximum number of supported Associations at the same time

- list of supported SOP Classes and Meta SOP Classes

- for each of the supported SOP and Meta SOP Classes:

- list of supported optional SOP Class Attributes and DIMSE Service Elements

- for each supported Attribute (mandatory and optional Attribute), the valid range of values

The SCP Conformance Statement shall specify the following items:

- maximum number of supported Associations at the same time

- list of supported SOP Classes and Meta SOP Classes

- minimum and maximum number of printable pixel matrix per supported film size

- for each of the supported SOP Classes:

- list of supported optional SOP Class Attributes and DIMSE Service Elements

- for each supported Attribute (mandatory and optional Attribute):

- valid range of values

- default value if no value is supplied by the SCU

- status code (Failure or Warning) if SCU supplies a value that is out of range

- for each supported DIMSE Service, the SCP behavior for all specific status codes

- description of each supported custom Image Display Format (2010,0010) e.g., position and dimensions of each composing image box, numbering scheme of the image positions

- description of each supported Annotation Display Format ID (2010,0030) e.g., position and dimensions of annotation box, font, number of characters

- description of each supported configuration table (e.g., identification, content)

- if the SCP supports N-ACTION for the Film Session SOP Class then the SCP shall specify the maximum number of collated films

- in the case of grayscale printers that print color images, the behavior of printing color images

- if cropping of images is supported, the algorithm for removing rows and columns from the image

Prev | Up | Next
H.3.3.2 List of Optional SOP Classes | Home | H.4 Print Management SOP Class Definitions

DICOM PS3.4 2017b - Service Class Specifications