DICOM PS3.16 2017b - Content Mapping Resource

Breast Imaging Report Templates
Prev | A Structured Reporting Templates (Normative) | Next

## Breast Imaging Report Templates

The Templates that comprise the Breast Imaging Report are interconnected as in Figure A-10.

Figure A-10. Breast Imaging Report Template Structure

### TID 4200 Breast Imaging Report

This Template forms the content tree that allows a Breast Imaging Report device to describe the results of a radiologist's diagnostic interpretation of Breast Imaging (e.g., X-Ray mammography or breast ultrasound) evidence. This Template, together with its subordinate Templates, describes the results for presentation to clinicians, or for consumption by Breast Imaging Report devices for subsequent Breast Imaging Reports.

This Template shall be instantiated at the Root node only.

See Figure Q.1-1 “Top Level of Breast Imaging Report Content Tree” in PS3.17 .

Type:

  Non-Extensible

Order:

  Significant

Root:

  Yes

Table TID 4200. Breast Imaging Report

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (111400, DCM, "Breast Imaging Report") | 1 | M |  | Root node
2 | > | HAS CONCEPT MOD | INCLUDE | DTID 1204 “Language of Content Item and Descendants” | 1 | M |  |
3 | > | CONTAINS | INCLUDE | DTID 4202 “Breast Imaging Report Narrative” | 1 | M |  |
4 | > | CONTAINS | INCLUDE | DTID 4208 “Breast Imaging Report Supplementary Data” | 1 | U |  |

Prev | Up | Next
TID 4129 Colon CAD Geometry | Home | TID 4201 Breast Imaging Procedure Reported

DICOM PS3.16 2017b - Content Mapping Resource