DICOM PS3.7 2017b - Message Exchange

7.5.3.2 Multiple Responses
Prev | 7.5.3 DIMSE Procedures | Next

#### 7.5.3.2 Multiple Responses

Each DIMSE service requires one or more response primitives as a result of the invocation of the service. How and when the multiple response primitives are used is defined by the procedures for the DIMSE service. Whether multiple responses are returned is conditional upon the information included in the request primitive by the DIMSE-service-user.

Prev | Up | Next
7.5.3 DIMSE Procedures | Home | 7.5.3.3 Cancellation

DICOM PS3.7 2017b - Message Exchange