DICOM PS3.4 2017e - Service Class Specifications

GG.6.3 Template Storage SOP Classes
Prev | GG.6 Application Behavior for Standard SOP Classes | Next

### GG.6.3 Template Storage SOP Classes

An implementation that is a Generic Implant Template Storage, Implant Assembly Template Storage, or Implant Template Group Storage SOP Class SCU may modify information in a SOP Instance that it has previously sent or received. When this SOP Instance is modified and sent to an SCP, it shall be assigned a new SOP Instance UID if there is addition, removal or update of any Attribute within:

- Generic Implant Template Description Module

- Generic Implant Template 2D Drawings Module

- Generic Implant Template 3D Models Module

- Generic Implant Template Mating Features Module

- Generic Implant Template Planning Landmarks Module

- Implant Assembly Template Module

- Implant Template Group Module

- Surface Mesh Module

Referential integrity between sets of related SOP instances shall be maintained.

Prev | Up | Next
GG.6.2.2 Display Application | Home | GG.6.4 CT Defined Procedure Protocol Storage SOP Class

DICOM PS3.4 2017e - Service Class Specifications