DICOM PS3.18 2017e - Web Services

6.2.2 Media Types Acceptable in the Response
Prev | 6.2 WADO-URI Request | Next

### 6.2.2 Media Types Acceptable in the Response

#### 6.2.2.1 Query Parameters

See Section 6.1.4.

##### 6.2.2.1.1 Accept Query Parameter

Specifies the Acceptable Media Types for the response payload. See Section 6.1.1.4. The name of the parameter is "contentType", which is case-sensitive. Its syntax is:

        accept = %s"contentType" "=" 1#rendered-media-type / 1#uri-media-type

The WADO-URI service supports Rendered Media Types (see Section 6.1.1.3) or the uri-media-type (see Section 6.1.1.8.5).

The transfer-syntax and charset media type parameters are forbidden in the request.

### Note

1. WADO-URI origin servers support transfer syntax and charset query parameters, which have been used instead of transfer-syntax and charset media type parameters since the inception of the service, even though this is different from the approach used by the later introduced WADO-RS service, which uses transfer-syntax and charset media type parameters instead of query parameters.

2. Only one transferSyntax query parameter is permitted and it may have only one UID value. See Section 8.2.11.

##### 6.2.2.1.2 Character Set Query Parameter

Specifies the Acceptable Character Sets for the response payload. See Section 6.1.2.1. The name of the parameter is "charset", which is case-sensitive. Its syntax is:

        charset-qp = %s"charset" "=" 1#(charset [weight])

Prev | Up | Next
6.2 WADO-URI Request | Home | 6.2.2.2 Header Fields

DICOM PS3.18 2017e - Web Services