DICOM PS3.4 2018a - Service Class Specifications

CC.2.7 Get Unified Procedure Step Information (N-GET)
Prev | CC.2 DIMSE Service Groups | Next

### CC.2.7 Get Unified Procedure Step Information (N-GET)

This operation allows an SCU to get information from an SCP about a specific real-world Procedure Step that is represented as a Unified Procedure Step Instance. This operation shall be invoked by the SCU through the DIMSE N-GET Service.

#### CC.2.7.1 Unified Procedure Step IOD Subset Specification

The Application Entity that claims conformance to the UPS Pull or UPS Watch SOP Classes as an SCU may choose to retrieve a subset of the Attribute values maintained by the SCP. The Application Entity that claims conformance as an SCP to these SOP Classes shall support the Attributes specified in Table CC.2.5-3.

Prev | Up | Next
CC.2.6.4 Status Codes | Home | CC.2.7.2 Service Class User Behavior

DICOM PS3.4 2018a - Service Class Specifications