DICOM PS3.3 2018a - Information Object Definitions

A.21 Positron Emission Tomography Image IOD
Prev | A Composite Information Object Definitions (Normative) | Next

## A.21 Positron Emission Tomography Image IOD

### A.21.1 PET Image IOD Description

The Positron Emission Tomography (PET) Image Information Object Definition specifies an image that has been created by a Positron Tomograph imaging device, including dedicated PET cameras and Nuclear Medicine imaging devices operating in coincidence mode. This includes data created by external detection devices that create images of the distribution of administered radioactive materials, specifically positron emitters, in the body. Depending on the specific radiopharmaceuticals administered and the particular imaging procedure performed, problems involving changes in metabolism, function, or physiology can be investigated and various region pathologies can be studied. For these problems, quantitation of image data in absolute activity and physiological units is important. In addition, the PET Image IOD specifies attenuation (transmission) images used for correction and anatomical reference of emission images.

Prev | Up | Next
A.20.3.4 RT Patient Setup Module | Home | A.21.2 PET Image IOD Entity-Relationship Model

DICOM PS3.3 2018a - Information Object Definitions