DICOM PS3.3 2018a - Information Object Definitions

A.32.4.3 VL Photographic Image IOD Content Constraints
Prev | A.32.4 VL Photographic Image IOD | Next

#### A.32.4.3 VL Photographic Image IOD Content Constraints

##### A.32.4.3.1 Modality

The value of Modality (0008,0060) shall be XC.

Prev | Up | Next
A.32.4.2 VL Photographic Image IOD Entity-Relationship Model | Home | A.32.5 Video Endoscopic Image IOD

DICOM PS3.3 2018a - Information Object Definitions