DICOM PS3.4 2018a - Service Class Specifications

O.3 Modification of SR Document Content
Prev | O Structured Reporting Storage SOP Classes (Normative) | Next

## O.3 Modification of SR Document Content

A device that is an SR Storage SOP Class SCU may modify information in a SOP Instance that it has previously sent or received. When this SOP Instance is modified and sent to an SCP, it shall be assigned a new SOP Instance UID if any of the following conditions are met:

- addition, removal or update of any Attribute within the SR Document General Module or SR Document Content Module;

- modification of the Series Instance UID (0020,000E);

- modification of the Study Instance UID (0020,000D).

Prev | Up | Next
O.2.2.2 Extensible SR SOP Class | Home | O.4 Conformance

DICOM PS3.4 2018a - Service Class Specifications