DICOM PS3.3 2018a - Information Object Definitions

C.8.14.3 MR Spectroscopy Functional Group Macros
Prev | C.8.14 MR Spectroscopy Modules | Next

#### C.8.14.3 MR Spectroscopy Functional Group Macros

The following sections contain Functional Group Macro's specific to the MR Spectroscopy IOD.

### Note

The attribute descriptions in the Functional Group Macros are written as if they were applicable to a single frame (i.e., the macro is part of the Per-frame Functional Groups Sequence). If an attribute is applicable to all frames (i.e., the macro is part of the Shared Functional Groups Sequence) the phrase "this frame" in the attribute description shall be interpreted to mean " for all frames".".

##### C.8.14.3.1 MR Spectroscopy Frame Type Macro

Table C.8-104 specifies the attributes of the MR Spectroscopy Frame Type Functional Group Macro.

Table C.8-104. MR Spectroscopy Frame Type Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
MR Spectroscopy Frame Type Sequence | (0018,9227) | 1 | Identifies sequence containing Frame Type Attributes. Only a single Item shall be included in this Sequence.
>Frame Type | (0008,9007) | 1 | Spectroscopy data characteristics. See Section C.8.14.5.1.1.
>Include Table C.8-107 “MR Spectroscopy Description Macro Attributes” |

Prev | Up | Next
C.8.14.2 MR Spectroscopy Pulse Sequence Module | Home | C.8.14.3.2 MR Spectroscopy FOV/Geometry Macro

DICOM PS3.3 2018a - Information Object Definitions