DICOM PS3.3 2018b - Information Object Definitions

A.35.7.2 Procedure Log IOD Entity-Relationship Model
Prev | A.35.7 Procedure Log IOD | Next

#### A.35.7.2 Procedure Log IOD Entity-Relationship Model

This IOD uses the E-R Model in Section A.1.2, with only the SR Document IE below the Series IE.

### Note

Unlike some other SR IODs, the Frame of Reference IE is critical to the synchronized time stamping of events in the Procedure Log IOD and to multi-modality coordination.

Prev | Up | Next
A.35.7 Procedure Log IOD | Home | A.35.7.3 Procedure Log IOD Module Table

DICOM PS3.3 2018b - Information Object Definitions