DICOM PS3.7 2018b - Message Exchange

C.5.15 Mistyped Argument
Prev | C.5 Failure Status Class | Next

### C.5.15 Mistyped Argument

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0212H.

Prev | Up | Next
C.5.14 Missing Attribute Value | Home | C.5.16 No Such Argument

DICOM PS3.7 2018b - Message Exchange