DICOM PS3.3 2018b - Information Object Definitions

C.8.14.5 MR Spectroscopy Description Macro
Prev | C.8.14 MR Spectroscopy Modules | Next

#### C.8.14.5 MR Spectroscopy Description Macro

Table C.8-107 specifies the Attributes that describe the Spectroscopy.

Table C.8-107. MR Spectroscopy Description Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Volumetric Properties | (0008,9206) | 1 | Indication if geometric manipulations are possible with frames in the SOP Instance. See Section C.8.14.5.1.2 for a description and Enumerated Values.
Volume Based Calculation Technique | (0008,9207) | 1 | Method used for volume calculations with frames in the SOP Instance. See Section C.8.14.5.1.3 for a description and Defined Terms.
Complex Image Component | (0008,9208) | 1 | Representation of complex data of frames in the SOP Instance. See Section C.8.14.5.1.4 for a description and Defined Terms.
Acquisition Contrast | (0008,9209) | 1 | Indication of acquisition contrast used with frames in the SOP Instance. See Section C.8.14.5.1.5 for a description and Defined Terms.

##### C.8.14.5.1 MR Spectroscopy Description Attribute Description

###### C.8.14.5.1.1 Image Type and Frame Type

Image Type (0008,0008) and Frame Type (0008,9007) are not included in this Macro but one or the other is always included in the Module or Macro that invokes this Macro, and they are therefore described here.

In addition to the requirements specified in Section C.8.16.1 Image Type and Frame Type, the following additional requirements and Defined Terms are specified.

###### C.8.14.5.1.1.1 Pixel Data Characteristics

See Section C.8.16.1.1. No additional requirements or Defined Terms.

###### C.8.14.5.1.1.2 Patient Examination Characteristics

See Section C.8.16.1.2. No additional requirements or Defined Terms.

###### C.8.14.5.1.1.3 Image Flavor

See Section C.8.16.1.3 for requirements, but not Defined Terms.

Table C.8-108 specifies the Defined Terms for MR Spectroscopy for Value 3 for Image Type (0008,0008) and Frame Type (0008,9007).

Table C.8-108. MR Spectroscopy Image Type and Frame Type Value 3

Defined Term Name | Defined Term Description
--- | ---
SPECTROSCOPY | Spectroscopy

###### C.8.14.5.1.1.4 Derived Pixel Contrast

See Section C.8.16.1.4 for requirements, but not Defined Terms.

Table C.8-109 specifies the Defined Terms for Value 4 for Image Type (0008,0008) and Frame Type (0008,9007).

Table C.8-109. MR Spectroscopy Image Type and Frame Type Value 4

Defined Term Name | Defined Term Description
--- | ---
ADDITION | Created through point by point addition operation
DIVISION | Created through point by point division operation
MAXIMUM | Created through point by point maximum operation
MEAN | Created through point by point mean operation
MINIMUM | Created through point by point minimum operation
MULTIPLICATION | Created through point by point multiplication operation
STD_DEVIATION | Standard Deviation
SUBTRACTION | Created through point by point subtraction operation
NONE | Not calculated
MIXED | Used only as value in Image Type (0008,0008) if frames within the spectroscopy SOP Instance contain different values for value 4 in their Frame Type (0008,9007) Attribute.

###### C.8.14.5.1.2 Volumetric Properties

See Section C.8.16.2.1.2. No additional requirements or Defined Terms.

###### C.8.14.5.1.3 Volume Based Calculation Technique Attribute

See Section C.8.16.2.1.3 for requirements, but not Defined Terms.

Table C.8-110 specifies the Defined Terms for the Volume Based Calculation Technique (0008,9207) Attribute.

Table C.8-110. Volume Based Calculation Technique Attribute Values

Defined Term Name | Defined Term Description
--- | ---
MAX_IP | Maximum Intensity Projection
MIN_IP | Minimum Intensity Projection
NONE | Pixels not derived geometrically
MIXED | Used only as a value in Volume Based Calculation Technique (0008,9207) Attribute in the MR Spectroscopy Module if frames within the image SOP Instance contain different terms for the Volume Based Calculation Technique Attribute in MR Spectroscopy Frame Type Functional Group.

###### C.8.14.5.1.4 Complex Image Component

The value of Complex Image Component (0008,9208) Attribute shall be used to indicate which component of the complex representation of the signal is represented in the spectroscopy data.

Table C.8-111 specifies the Defined Terms for Complex Image Component (0008,9208).

Table C.8-111. Complex Image Component Attribute Values

Defined Term Name | Defined Term Description
--- | ---
MAGNITUDE | The magnitude component of the complex spectroscopy data.
PHASE | The phase component of the complex spectroscopy data.
REAL | The real component of the complex spectroscopy data.
IMAGINARY | The imaginary component of the complex spectroscopy data.
COMPLEX | The real and imaginary components of the complex spectroscopy data
MIXED | Used only as a value in Complex Image Component (0008,9208) in the MR Spectroscopy Module if frames within the image SOP Instance contain different values for the Complex Image Component Attribute in the MR Spectroscopy Frame Type Functional Group.

###### C.8.14.5.1.5 Acquisition Contrast

Table C.8-112 specifies the Defined Terms for Acquisition Contrast (0008,9209).

Table C.8-112. Acquisition Contrast Values

Defined Term Name | Defined Term Description
--- | ---
PROTON_DENSITY | Proton Density weighted contrast
T1 | T1 weighted contrast
T2 | T2 weighted contrast
UNKNOWN | Value should be UNKNOWN if acquisition contrasts were combined resulting in an unknown contrast. Also this value should be used when the contrast is not known.
MIXED | Used only as a value in Acquisition Contrast (0008,9209) Attribute in the MR Spectroscopy Module if frames within the SOP Instance contain different values for the Acquisition Contrast Attribute in the MR Spectroscopy Frame Type Functional Group.

Prev | Up | Next
C.8.14.4 MR Spectroscopy Data Module | Home | C.8.15 Enhanced CT Image

DICOM PS3.3 2018b - Information Object Definitions