DICOM PS3.11 2018b - Media Storage Application Profiles

I.3.2 Physical Medium and Medium Format
Prev | I.3 STD-DVD-MPEG2-MPML and STD-DVD-SEC-MPEG2-MPML Profile Classes | Next

### I.3.2 Physical Medium and Medium Format

The STD-DVD-MPEG2-MPML and STD-DVD-SEC-MPEG2-MPML application profiles require any of the 120 mm DVD media other than DVD-RAM, as defined in PS3.12.

Prev | Up | Next
I.3 STD-DVD-MPEG2-MPML and STD-DVD-SEC-MPEG2-MPML Profile Classes | Home | I.3.3 Directory Information in DICOMDIR

DICOM PS3.11 2018b - Media Storage Application Profiles