DICOM PS3.16 2018d - Content Mapping Resource

TID 3714 ECG Lead Measurements (Current)
Prev | ECG Report Templates | Next

### TID 3714 ECG Lead Measurements

The ECG Lead Measurements Template provides a structure for measurements calculated on individual ECG leads.

As an Extensible Template, applications may include any ECG per lead measurements, such as integrals over time of various ECG wave voltages. The recommended vocabulary for such concepts is ISO/IEEE 11073-10102.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 3714. ECG Lead Measurements

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (122159, DCM, "ECG Lead Measurements") | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (122148, DCM, "Lead ID") | 1 | M |  | BCID 3001 “ECG Leads”
3 | > | HAS OBS CONTEXT | INCLUDE | DTID 3715 “ECG Measurement Source” | 1 | U |  |
4 | > | CONTAINS | NUM | DCID 3687 “Electrophysiology Waveform Durations” | 1-n | U |  | UNITS = EV (ms, UCUM, "ms")
5 | > | CONTAINS | NUM | DCID 3688 “Electrophysiology Waveform Voltages” | 1-n | U |  | UNITS = EV (mV, UCUM, "mV")
6 | > | CONTAINS | CODE | EV (F-38035, SRT, "ST Segment Finding") | 1 | U |  | DCID 3233 “ST Segment Morphology”
7 | > | CONTAINS | CODE | EV (121071, DCM, "Finding") | 1-n | U |  | DCID 3680 “ECG Lead Noise Descriptions”

Prev | Up | Next
TID 3713 ECG Global Measurements | Home | TID 3715 ECG Measurement Source

DICOM PS3.16 2018d - Content Mapping Resource