DICOM PS3.5 2018d - Data Structures and Encoding

A.4.10 HEVC/H.265 Main 10 Profile / Level 5.1 Video Compression (Current)
Prev | A.4 Transfer Syntaxes For Encapsulation of Encoded Pixel Data | Next

### A.4.10 HEVC/H.265 Main 10 Profile / Level 5.1 Video Compression

The International Standards Organization ISO/IEC MPEG has developed an International Standard, [ISO/IEC 23008-2] (HEVC), for the video compression of generic coding of moving pictures and associated audio information. This standard is jointly maintained and has identical technical content as the [ISO/IEC 23008-2] HEVC standard.

A DICOM Transfer Syntax for HEVC/H.265 Main 10 Profile / Level 5.1 Video Compression shall be identified by a UID value of:

- 1.2.840.10008.1.2.4.108 corresponding to the HEVC/H.265 Main 10 Profile / Level 5.1 of the [ISO/IEC 23008-2] HEVC Video standard.

Prev | Up | Next
A.4.9 HEVC/H.265 Main Profile / Level 5.1 Video Compression | Home | A.5 DICOM Deflated Little Endian Transfer Syntax (Explicit VR)

DICOM PS3.5 2018d - Data Structures and Encoding