DICOM PS3.4 2018d - Service Class Specifications

P.2.5.2 SCP Conformance (Current)
Prev | P.2.5 Conformance Requirements | Next

#### P.2.5.2 SCP Conformance

The SCP shall document in its Conformance Statement how it uses the identifiers it receives for matching the N-ACTION (Procedural Event Notification) to a specific procedure.

The SCP shall document the behavior and actions that cause the SCP to generate a success, warning, or failure status for a received N-ACTION.

The SCP shall document the behavior and actions that cause the SCP to generate a Procedure Log SOP Instance including the received Event Information.

The SCP shall document how it assigns the value of the Observation Datetime (0040,A032) Attribute when the SCU-provided Synchronization Frame of Reference UID is absent, or differs from that of the SCP.

Prev | Up | Next
P.2.5 Conformance Requirements | Home | P.3 Substance Administration Logging SOP Class Definition

DICOM PS3.4 2018d - Service Class Specifications