DICOM PS3.11 2018d - Media Storage Application Profiles

G.3 STD-GEN-MIME Profile (Current)
Prev | G General Purpose MIME Interchange Profile (Normative) | Next

## G.3 STD-GEN-MIME Profile

### G.3.1 SOP Classes and Transfer Syntaxes

This Application Profile is based on the Media Storage Service Class (see PS3.4).

Table G.3-1. STD-GEN-MIME SOP Classes and Transfer Syntaxes

Information Object Definition | SOP Class UID | Transfer Syntax and UID | FSC Requirement | FSR Requirement
--- | --- | --- | --- | ---
Basic Directory | 1.2.840.10008.1.3.10 | Explicit VR Little Endian Uncompressed 1.2.840.10008.1.2.1 | Optional | Optional
Composite Image & Stand-alone Storage | See PS3.4 | Defined in Conformance Statement | Defined in Conformance Statement | Defined in Conformance Statement

The SOP Classes and corresponding Transfer Syntax supported by this Application Profile are specified in the Table G.3-1. The supported Storage SOP Class(es) and Transfers Syntax(es) shall be listed in the Conformance Statement using a table of the same form.

Prev | Up | Next
G.2.1.2 File Set Reader | Home | G.3.2 Physical Medium and Medium Format

DICOM PS3.11 2018d - Media Storage Application Profiles