DICOM PS3.17 2018d - Explanatory Information

LL Example SCU Use of The Composite Instance Root Retrieval Classes (Informative) (Current)
Prev |  | Next

# LL Example SCU Use of The Composite Instance Root Retrieval Classes (Informative)

## LL.1 Retrieval of Entire Composite Instances

There are many modules in DICOM that use the Image SOP Instance Reference Macro (Table 10-3 “Image SOP Instance Reference Macro Attributes” in PS3.3 ), which includes the SOP Instance UID and SOP class UID, but not the Series Instance UID and Study Instance UID. Using the Composite Instance Root Retrieval Classes however, retrieval of such instances is simple, as a direct retrieval may be requested, including only the SOP Instance UID in the Identifier of the C-GET request.

Prev |  | Next
KK.5 Independent WADO Server | Home | LL.2 Retrieval of Selected Frame Composite Instances From Multi-frame Objects

DICOM PS3.17 2018d - Explanatory Information