DICOM PS3.3 2018d - Information Object Definitions

C.34.9.3 Attribute Value Constraint Macro (Current)
Prev | C.34.9 Defined CT Acquisition Module | Next

#### C.34.9.3 Attribute Value Constraint Macro

The CT Defined Procedure Protocol SOP Class assigns the following significance to the values of Constraint Violation Significance (0082,0036) :

- FAILURE - Violating the constraint is a violation of the Protocol and requires supervisory permission and auditing.

- WARNING - Violating the constraint is a violation of the Protocol and requires operator confirmation and auditing.

- INFORMATIVE - Violating the constraint is not a violation of the Protocol. The constraint represents a guideline. Violation of the guideline may be recorded or shown to the operator.

If the Attribute is absent, a value of INFORMATIVE may be assumed.

Prev | Up | Next
C.34.9.2 Dose Related Attributes in Parameter Specification Sequence | Home | C.34.9.4 Modifiable Constraint Flag

DICOM PS3.3 2018d - Information Object Definitions