DICOM PS3.4 2018d - Service Class Specifications

U.2 Hanging Protocol Information Model Definition (Current)
Prev | U Hanging Protocol Query/Retrieve Service Class | Next

## U.2 Hanging Protocol Information Model Definition

The Hanging Protocol Information Model is identified by the SOP Class negotiated at Association establishment time. The SOP Class is composed of both an Information Model and a DIMSE-C Service Group.

The Hanging Protocol Information Model is defined, with the Entity-Relationship Model Definition and Key Attributes Definition analogous to those defined in the Worklist Information Model Definition of the Basic Worklist Management Service.

Prev | Up | Next
U Hanging Protocol Query/Retrieve Service Class | Home | U.3 Hanging Protocol Information Model

DICOM PS3.4 2018d - Service Class Specifications