DICOM PS3.4 2018d - Service Class Specifications

CC.2.5.4 Status Codes (Current)
Prev | CC.2.5 Create a Unified Procedure Step (N-CREATE) | Next

#### CC.2.5.4 Status Codes

Table CC.2.5-4 defines the status code values that might be returned in a N-CREATE response. General status code values and fields related to status code values are defined for N-CREATE DIMSE Service in PS3.7.

Table CC.2.5-4. Status Values

Service Status | Further Meaning | Status Code
--- | --- | ---
Success | The UPS was created as requested | 0000
Warning | The UPS was created with modifications | B300
Failure | Failed: The provided value of UPS State was not "SCHEDULED". | C309

Prev | Up | Next
CC.2.5.3 Service Class Provider Behavior | Home | CC.2.6 Set Unified Procedure Step Information (N-SET)

DICOM PS3.4 2018d - Service Class Specifications