DICOM PS3.16 2018d - Content Mapping Resource

CID 3687 Electrophysiology Waveform Durations (Current)
Prev | B DCMR Context Groups (Normative) | Next

## CID 3687 Electrophysiology Waveform Durations

This Context Group consists of the per-lead terms under the hierarchy of Reference ID MDC_ECG_TIME_PD in the ISO/IEEE 11073-10102 nomenclature.

The base terms from that hierarchy are included in the table below for reference. The per-lead base terms are pre-coordinated with concept discriminators for specific leads, and the code values for those pre-coordinated terms are arithmetically derived from the code values of the base terms. For the complete current list of terms and discriminator values, see the ISO/IEEE Standard. All pre-coordinated terms (measurements plus discriminators) within the identified hierarchy are part of this Context Group.

### Note

1. A prior version of this context group used codes from the SCP-ECG coding system.

2. Codes reprinted by permission of IEEE, Copyright 2004 by IEEE. ISO/IEEE 11073-10102 available through http://standards.ieee.org/.

Resources:

  HTML | FHIR JSON | FHIR XML | IHE SVS XML

Type:

  Extensible

Version:

  20110330

UID:

  1.2.840.10008.6.1.201

Table CID 3687. Electrophysiology Waveform Durations

Coding Scheme Designator | Code Value | Code Meaning | ISO/IEEE 11073 MDC Equivalent Reference ID (Informative)
--- | --- | --- | ---
MDC | 2:6656 | P duration, per lead | MDC_ECG_TIME_PD_P
MDC | 2:4608 | P onset to P1 duration, per lead | MDC_ECG_TIME_PD_P1
MDC | 2:4864 | P onset to P2 duration, per lead | MDC_ECG_TIME_PD_P2
MDC | 2:5120 | P onset to P3 duration, per lead | MDC_ECG_TIME_PD_P3
MDC | 2:7168 | P offset to QRS onset duration, per lead | MDC_ECG_TIME_PD_PR
MDC | 2:7680 | Q duration, per lead | MDC_ECG_TIME_PD_Q
MDC | 2:7936 | QRS duration, per lead | MDC_ECG_TIME_PD_QRS
MDC | 2:8192 | QT duration, per lead | MDC_ECG_TIME_PD_QT
MDC | 2:11264 | R1 duration, per lead | MDC_ECG_TIME_PD_R_1
MDC | 2:11520 | R2 duration, per lead | MDC_ECG_TIME_PD_R_2
MDC | 2:11776 | R3 duration, per lead | MDC_ECG_TIME_PD_R_3
MDC | 2:12032 | S1 duration, per lead | MDC_ECG_TIME_PD_S_1
MDC | 2:12288 | S2 duration, per lead | MDC_ECG_TIME_PD_S_2
MDC | 2:12544 | S3 duration, per lead | MDC_ECG_TIME_PD_S_3
MDC | 2:11008 | Ventricular activation time, per lead | MDC_ECG_TIME_PD_VENT_ACTIV
MDC | 2:32768 | PP time period, per lead | MDC_ECG_TIME_PD_PP
MDC | 2:33024 | RR time period, per lead | MDC_ECG_TIME_PD_RR
MDC | 2:33280 | PQ time period, per lead | MDC_ECG_TIME_PD_PQ
MDC | 2:33536 | PQ segment time period, per lead | MDC_ECG_TIME_PD_PQ_SEG
MDC | 2:34560 | QTU time period, per lead | MDC_ECG_TIME_PD_QTU

Prev | Up | Next
CID 3686 ECG Interpretive Statements (Retired) | Home | CID 3688 Electrophysiology Waveform Voltages

DICOM PS3.16 2018d - Content Mapping Resource