DICOM PS3.17 2018d - Explanatory Information

C.5 Waveform Information Model (Current)
Prev | C Waveforms (Informative) | Next

## C.5 Waveform Information Model

The part of the composite information object that carries the waveform data is the Waveform Information Entity (IE). The Waveform IE includes the technical parameters of waveform acquisition and the waveform samples.

The information model, or internal organizational structure, of the Waveform IE is shown in Figure C.5-1. A waveform information object includes data from a continuous time period during which signals were acquired. The object may contain several multiplex groups, each defined by digitization with the same clock whose frequency is defined for the group. Within each multiplex group there will be one or more channels, each with a full technical definition. Finally, each channel has its set of digital waveform samples.

Figure C.5-1. DICOM Waveform Information Model

Prev | Up | Next
C.4 Waveform Acquisition Model | Home | C.6 Harmonization With HL7

DICOM PS3.17 2018d - Explanatory Information