DICOM PS3.3 2018d - Information Object Definitions

C.7.6.4b Enhanced Contrast/Bolus Module (Current)
Prev | C.7.6 Common Image IE Modules | Next

#### C.7.6.4b Enhanced Contrast/Bolus Module

Table C.7-12b specifies the Attributes that describe the contrast/bolus used in the acquisition of the Image.

Table C.7-12b. Enhanced Contrast/Bolus Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Contrast/Bolus Agent Sequence | (0018,0012) | 1 | Sequence that identifies one or more contrast agents administered prior to or during the acquisition. One or more Items shall be included in this Sequence.
>Include Table 8.8-1 “Code Sequence Macro Attributes” | Baseline CID 12 “Radiographic Contrast Agent”.
>Contrast/Bolus Agent Number | (0018,9337) | 1 | Identifying number, unique within this SOP Instance, of the agent administered. Used to reference this particular agent from the Contrast/Bolus Functional Group Macro. The number shall be 1 for the first Item and increase by 1 for each subsequent Item.
>Contrast/Bolus Administration Route Sequence | (0018,0014) | 1 | Sequence that identifies the route of administration of contrast agent. Only a single Item shall be included in this Sequence.
>>Include Table 8.8-1 “Code Sequence Macro Attributes” | Baseline CID 11 “Route of Administration”.
>Contrast/Bolus Ingredient Code Sequence | (0018,9338) | 2 | Active ingredient of agent. Zero or more Items shall be included in this Sequence.
>>Include Table 8.8-1 “Code Sequence Macro Attributes” | Baseline CID 13 “Radiographic Contrast Agent Ingredient”.
>Contrast/Bolus Volume | (0018,1041) | 2 | Total volume administered in milliliters of diluted contrast agent.
>Contrast/Bolus Ingredient Concentration | (0018,1049) | 2 | Milligrams of active ingredient per milliliter of agent.
>Contrast/Bolus Ingredient Percent by Volume | (0052,0001) | 3 | Percentage by volume of active ingredient in the total volume.
>Contrast/Bolus Ingredient Opaque | (0018,9425) | 3 | Absorption of the ingredient greater than the absorption of water (tissue). Enumerated Values: YES NO See Section C.7.6.4b.1.
>Contrast/Bolus T1 Relaxivity | (0018,0013) | 3 | T1 Relaxivity of the MR Contrast/Bolus used specified in s-1*mmol-1 specified at body temperature in human blood plasma.
>Contrast Administration Profile Sequence | (0018,9340) | 3 | Sequence that describes one or more phases of contrast administered. One or more Items are permitted in this Sequence.
>>Contrast/Bolus Volume | (0018,1041) | 2 | Volume administered during this phase in milliliters of diluted contrast agent.
>>Contrast/Bolus Start Time | (0018,1042) | 3 | Time of start of administration.
>>Contrast/Bolus Stop Time | (0018,1043) | 3 | Time of end of administration.
>>Contrast Flow Rate | (0018,1046) | 3 | Rate of administration in milliliters/sec. Only a single value shall be present.
>>Contrast Flow Duration | (0018,1047) | 3 | Duration of injection in seconds. Only a single value shall be present.

##### C.7.6.4b.1 Enhanced Contrast/Bolus Module Attributes

###### C.7.6.4b.1.1 Contrast/Bolus Ingredient Opaque for X-Ray Equipment

Contrast/Bolus Ingredient Opaque (0018,9425) Attribute specifies the type of relative X-Ray absorption of the contrast/bolus ingredient, compared to the X-Ray absorption of water.

Enumerated Values:

YES

  The contrast/bolus ingredient absorbs more X-Ray photons than water

NO

  The contrast/bolus ingredient absorbs less X-Ray photons than water

### Note

The Contrast/Bolus Ingredient Opaque (0018,9425) Attribute determines the sign of the gradient of X-Ray beam intensity from inside to outside the injected vessel, thus allowing optimal settings of the image processing applications (e.g., vessel edge detection, etc.), see Figure C.7.6.4b-1.

The relative gray level of the injected vessel with respect to the gray level of the water of Pixel Data (7FE0,0010) is determined by the Contrast/Bolus Ingredient Opaque (0018,9425) and by the Pixel Intensity Relationship Sign (0028,1041). For example, if the contrast/bolus ingredient is more radio graphically dense than water (i.e., YES), and the Pixel Intensity Relationship Sign (0028,1041) is -1, then the contrast/bolus ingredient is represented by higher values of Pixel Data than water.

Figure C.7.6.4b-1. X-Ray beam intensity vs. Contrast/Bolus Ingredient Opaque

Prev | Up | Next
C.7.6.4 Contrast/Bolus Module | Home | C.7.6.5 Cine Module

DICOM PS3.3 2018d - Information Object Definitions