DICOM PS3.2 2018d - Conformance

G.4.3.2 Additional Protocols (Current)
Prev | G.4.3 Network Interfaces | Next

#### G.4.3.2 Additional Protocols

When host names rather than IP addresses are used in the configuration properties to specify presentation addresses for remote AEs, the application is dependent on the name resolution mechanism of the underlying operating system.

Prev | Up | Next
G.4.3 Network Interfaces | Home | G.4.3.3 IPv4 and IPv6 Support

DICOM PS3.2 2018d - Conformance