DICOM PS3.16 2018d - Content Mapping Resource

CID 4015 View Modifier for Mammography (Current)
Prev | B DCMR Context Groups (Normative) | Next

## CID 4015 View Modifier for Mammography

Resources:

  HTML | FHIR JSON | FHIR XML | IHE SVS XML

Type:

  Non-Extensible

Version:

  20090717

UID:

  1.2.840.10008.6.1.299

Table CID 4015. View Modifier for Mammography

Coding Scheme Designator | Code Value | Code Meaning | SNOMED-CT Concept ID | UMLS Concept Unique ID | Applies only when View ACR MQCM 1999 Equivalent is: | ACR MQCM 1999 Equivalent
--- | --- | --- | --- | --- | --- | ---
SRT | R-102D2 | Cleavage | 399161006 | C1302232 | CC or FB | CV
SRT | R-102D1 | Axillary Tail | 399011000 | C1302167 | MLO | AT
SRT | R-102D3 | Rolled Lateral | 399197002 | C1275832 | any | ...RL
SRT | R-102D4 | Rolled Medial | 399226006 | C1275838 | any | ...RM
SRT | R-102CA | Rolled Inferior | 414493004 | C1532323 | any | ...RI
SRT | R-102C9 | Rolled Superior | 415670009 | C1531911 | any | ...RS
SRT | R-102D5 | Implant Displaced | 399209000 | C1275834 | any | ...ID
SRT | R-102D6 | Magnification | 399163009 | C1302233 | any | M...
SRT | R-102D7 | Spot Compression | 399055006 | C1302185 | any | S...
SRT | R-102C2 | Tangential | 399110001 | C0442227 | any | TAN
SRT | R-40AB3 | Nipple in profile | 442581004 | C2711408 | any | ...NP
SRT | P2-00161 | Anterior compression | 441752004 | C2711933 | any | ...AC
SRT | R-40ABE | Infra-mammary fold | 442593008 | C2711136 | any | ...IMF
SRT | R-40AB2 | Axillary tissue | 442580003 | C2711122 | any | ...AX

### Note

1. The View ACR MQCM 1999 Equivalent is defined in CID 4014 “View for Mammography”.

2. Some applications and View Modifier ACR MQCM 1999 equivalents have been extended by DICOM to incorporate additional known clinical use cases. The View Modifier ACR MQCM 1999 equivalent indicates its use as a prefix (shown by trailing "…") or suffix (shown by preceding "…") to the View ACR MQCM 1999 equivalent, or replacement for the View ACR MQCM 1999 equivalent.

3. While SRT is the preferred Coding Scheme Designator for SNOMED, regulatory approval of mammography systems makes changes to such systems problematic. Implementers should be aware that many systems will continue to use the deprecated designator SNM3 for certain terms in this context group. It is recommended that implementations receiving Mammography Image or CAD SOP Instances support both SNM3 and SRT as equivalent Coding Scheme Designators for Attributes or Content Items that use this Context Group.

Prev | Up | Next
CID 4014 View for Mammography | Home | CID 4016 Anatomic Region for Intra-oral Radiography

DICOM PS3.16 2018d - Content Mapping Resource