DICOM PS3.2 2018e - Conformance

G.1 Conformance Statement Overview (Current)
Prev | G Conformance Statement Sample ImageViewer with Hanging Protocol Support (Informative) | Next

## G.1 Conformance Statement Overview

The application supports accepting Images and Presentation States from remote systems, and querying a remote system for Hanging Protocol Instances that may then be retrieved to the local system. It also supports sending locally loaded images and created Presentation State and Hanging Protocol Instances across the network to remote systems.

Table G.1-1. Network Services

SOP Classes | User of Service(SCU) | Provider of Service(SCP)
--- | --- | ---
Transfer |  |
Ultrasound Image Storage | Yes | Yes
Ultrasound Multi-frame Image Storage | Yes | Yes
MR Image Storage | Yes | Yes
Digital Mammography X-Ray Image Storage - For Presentation | Yes | Yes
Grayscale Softcopy Presentation State Storage SOP Class | Yes | Yes
Hanging Protocol Storage | Yes | Yes
Query/Retrieve |  |
Hanging Protocol Information Model - FIND | Yes | No
Hanging Protocol Information Model - MOVE | Yes | No

Prev | Up | Next
G Conformance Statement Sample ImageViewer with Hanging Protocol Support (Informative) | Home | G.2 Table of Contents

DICOM PS3.2 2018e - Conformance