DICOM PS3.11 2018e - Media Storage Application Profiles

C.3.2 Physical Media and Media Formats (Current)
Prev | C.3 General Class Profile | Next

### C.3.2 Physical Media and Media Formats

An ultrasound application profile class may be supported by any one of the media described in Table C.3-3.

Table C.3-3. Media Classes

Media | Media Classes | Media Format | PS3.12
2.3GB 90mm MOD | MOD23-90 | DOS, unpartitioned (removable media) | Annex Q “90 mm 2.3 GB Magneto-Optical Disk (Normative)”
CD-R | CDR | ISO/IEC 9660 | Annex F “120mm CD-R Medium (Normative)”
DVD-RAM | DVD-RAM | UDF1.5 | Annex J “UDF on 120 mm DVD-RAM Medium (Normative)”
120 mm DVD | DVD | UDF or ISO 9660 | Annex P “120 mm DVD Medium (Normative)”

### Note

Media Classes FLOP, MOD128, MOD230, MOD540, MOD640, MOD650, MOD12 AND MOD23 were previously defined but have been retired. See PS3.11 2004.

Prev | Up | Next
C.3 General Class Profile | Home | C.3.3 DICOMDIR

DICOM PS3.11 2018e - Media Storage Application Profiles